# time flashrom-usb -p ch341a_spi -r IS25LP064A.bin
flashrom v1.2.1 on Linux 4.14.221 (mips)
flashrom is free software, get the source code at https://flashrom.org

Calibrating delay loop... OK.
Found ISSI flash chip "IS25LP064" (8192 kB, SPI) on ch341a_spi.
===
This flash part has status UNTESTED for operations: PROBE READ ERASE WRITE
The test status of this chip may have been updated in the latest development
version of flashrom. If you are running the latest development version,
please email a report to flashrom@flashrom.org if any of the above operations
work correctly for you with this flash chip. Please include the flashrom log
file for all operations you tested (see the man page for details), and mention
which mainboard or programmer you tested in the subject line.
Thanks for your help!
Reading flash... done.
real	1m 6.48s
user	0m 9.44s
sys	0m 12.96s
# time flashrom-usb -p ch341a_spi -r IS25LP064A.bin
flashrom v1.2.1 on Linux 4.14.221 (mips)
flashrom is free software, get the source code at https://flashrom.org

Calibrating delay loop... OK.
Found ISSI flash chip "IS25LP064" (8192 kB, SPI) on ch341a_spi.
===
This flash part has status UNTESTED for operations: PROBE READ ERASE WRITE
The test status of this chip may have been updated in the latest development
version of flashrom. If you are running the latest development version,
please email a report to flashrom@flashrom.org if any of the above operations
work correctly for you with this flash chip. Please include the flashrom log
file for all operations you tested (see the man page for details), and mention
which mainboard or programmer you tested in the subject line.
Thanks for your help!
Reading flash... done.
real	1m 6.44s
user	0m 8.98s
sys	0m 14.78s
# time flashrom-usb -p ch341a_spi -E
flashrom v1.2.1 on Linux 4.14.221 (mips)
flashrom is free software, get the source code at https://flashrom.org

Calibrating delay loop... OK.
Found ISSI flash chip "IS25LP064" (8192 kB, SPI) on ch341a_spi.
===
This flash part has status UNTESTED for operations: PROBE READ ERASE WRITE
The test status of this chip may have been updated in the latest development
version of flashrom. If you are running the latest development version,
please email a report to flashrom@flashrom.org if any of the above operations
work correctly for you with this flash chip. Please include the flashrom log
file for all operations you tested (see the man page for details), and mention
which mainboard or programmer you tested in the subject line.
Thanks for your help!
Erasing and writing flash chip... Erase/write done.
real	3m 8.14s
user	2m 10.47s
sys	0m 13.35s
# time flashrom-usb -p ch341a_spi -r IS25LP064A.bin
flashrom v1.2.1 on Linux 4.14.221 (mips)
flashrom is free software, get the source code at https://flashrom.org

Calibrating delay loop... OK.
Found ISSI flash chip "IS25LP064" (8192 kB, SPI) on ch341a_spi.
===
This flash part has status UNTESTED for operations: PROBE READ ERASE WRITE
The test status of this chip may have been updated in the latest development
version of flashrom. If you are running the latest development version,
please email a report to flashrom@flashrom.org if any of the above operations
work correctly for you with this flash chip. Please include the flashrom log
file for all operations you tested (see the man page for details), and mention
which mainboard or programmer you tested in the subject line.
Thanks for your help!
Reading flash... done.
real	1m 6.47s
user	0m 9.69s
sys	0m 13.78s
